To install Wings to a hard drive:

  1.  Boot your hard drive normally and go to the WorkBench.
  2.  Insert Wings Reel 2 into any drive.
  3.  Double-click on the "Reel 2" disk icon.
  4.  Double-click on the icon named "HDInstall"
  5.  You should be prompted for the pathname on your hard drive where
      you wish to install Wings.  Enter the path name using double quotes.
      Example: "DH0:Wings".
  6.  The contents of Reel 2 will be transfered to your hard drive. When
      prompted, insert Reel 1 in any drive.
  7.  The contents of Reel 1 will be transfered to your hard drive. When
      the screen reads "Installation Complete" you should be set to play.

To play Wings from a hard drive:

  1.  Remove any Wings diskettes, if they are inserted.
  2.  Boot your hard drive normally and go to the WorkBench.
  3.  Double-click on the hard drive's icon.
  4.  Double-click on the icon with the name you gave it in step 5 above.
  5.  Double-click on the icon named "Wings".  The game should start.

      Notes on Hard Disk Installation for Amigas with 512K of Chip Ram

  The Wings program requires at least 1 Megabyte of memory and uses the
Amiga's graphics memory (chip ram) resources to the maximum extent possible.
If your Amiga has only 512K of chip ram (such as an A1000, or an A500 or
A2000 without the "Super Agnus" chip set) you may only be able to play
Wings off of the floppy disks (depending on your particular Amiga setup).

                      Tips to Minimize Chip Ram Usage

  Make sure that your S:STARTUP-SEQUENCE script loads only the files that
are needed for hard disk operation (i.e.  don't start unneeded programs,
create a RAM: disk, multi-task other applications etc.).

  Make sure that all open windows are closed so that the WorkBench can be
closed.

  Disconnect any external disk drives that may be connected (make sure the
power is off first!).

  If these attempts fail (or are too confusing) you can still play Wings
from the floppies.
         RAM: Disk Installation for Amigas with 3 Megabytes of Ram

  Use the HDInstall icon and specify a pathname such as "RAM:Wings" and the
game will install to the RAM: disk.  The same cautions about chip ram still
apply and you will need to copy the "Reel 2/pilot.dat" file to a floppy to
keep your saved game after the Amiga is powered off (and copy it back next
time after you install Wings).

  When installing to RAM: here is a handy trick to save enough chip ram: 

1.  Boot your Workbench disk.
2.  As soon as you see the CLI window appear press CTRL-D to stop the
    Startup-sequence.
3.  Type "LoadWB" and press RETURN.
4.  Type "EndCLI" and press RETURN.
5.  Insert "Reel 2" and double-click on its icon.
6.  Double-click on the "HDInstall" icon. Install to "RAM:Wings".
7.  Remove all Wings diskettes.
8.  Double-click on the RAM: icon.
9.  Double-click on the Wings drawer and then double-click on the Wings
    icon.
