



; bank 0x0C of 16 starts at file address 0x030010
; code bytes:	$0000 (0.00% of bytes in this ROM bank)
; data bytes:	$0000 (0.00% of bytes in this ROM bank)
; pcm bytes:	$0000 (0.00% of bytes in this ROM bank)
; chr bytes:	$0000 (0.00% of bytes in this ROM bank)
; free bytes:	$4000 (100.00% of bytes in this ROM bank)
; unknown bytes:	$0000 (0.00% of bytes in this ROM bank)

; [bank start] -> free
0x030010|$0C:$8000:FF
; ... skipping $3FFE FF bytes
0x03400F|$0C:$BFFF:FF