



; bank 0x0E of 16 starts at file address 0x038010
; code bytes:	$0000 (0.00% of bytes in this ROM bank)
; data bytes:	$0000 (0.00% of bytes in this ROM bank)
; pcm bytes:	$0000 (0.00% of bytes in this ROM bank)
; chr bytes:	$0000 (0.00% of bytes in this ROM bank)
; free bytes:	$4000 (100.00% of bytes in this ROM bank)
; unknown bytes:	$0000 (0.00% of bytes in this ROM bank)

; [bank start] -> free
0x038010|$0E:$8000:FF
; ... skipping $3FFE FF bytes
0x03C00F|$0E:$BFFF:FF