0240 vs 0252
to 0x920 same (header data, bitmaps info)
from 0x2D20 to 0x75D0 same (bitmap pointers, some palettes)
from 0x895D0 same (some bitmaps)
=> header/pointers same, some palettes/bitmaps differ


All data aligned to 16 bytes

-----------------------------------

0x0     Pointers to sections, "29002900" is end pointer?
0x0     zeros
0x4     Pointer to Data for images (1 entry 32 bytes, from 0xC - 2B width, 2B height, 4B bitmap size)
0x8     Pointer to Data for images (same 0x4)
0xC     Pointer to Data for images (1 entry 16 bytes, unknow (order? depths?)
0x10>=  Pointer to "data section start" (some are same, some are zeros)


0x810   "data section start", 16bytes zeros
0x818   pointer to "bitmap pointers" from section start
0x81C   pointer to "palette pointers" from section start
0x870   "palette pointers", base "data section start" (0x810)
        44 pointes, some empty (zero)

0x920   first palette start


0x7520  "bitmap pointers", 44 pointes, some empty (zero)
        Start from "0x6DC0" -> Base "data section start" (0x810).
        First 3 images size 0x10000 - 256x256x8, others different

0x75D0  first bitmap start

0x9A1D0 graphic index 33 (34th), graphic S.Lvl, 128*128*8 = 0x4000 bytes (16384 bytes)
        (132th byte in header)
        (palette from 0x5920)

