##command:AFter EVent
##Event that occurs after another event has happened.
AFEV, 1, 12, -language:FE8:FE7:FE6 -priority:main -indexMode:8
##Once the event ID has been marked as 'used', this event can't be invoked.
##Leaving this as 0 will allow the event to occur whenever otherwise possible.
	EventID, 2, 2
##The event which is to occur.
	EventPointer, 4, 4, -pointer
##The event ID of the previous event to follow up on.
	PreviousEventID, 8, 2

AFEV, 0, 4, -priority:main -language:FE8:FE7:FE6 -end -indexMode:8 -noDisassembly
	0, 0, 4, -fixed