*************************************
* ERX308 for Z80 2.21 Release Notes *
*************************************

February 19, 1993

FILES

     README.1ST     This file
     INSTALL.BAT    Batch file for software installation
     ERXZ80.EXE     Emulator executable file.
     ERXZ80.HLP     Help file
     ERXZ80.MAC     Standard macro file
     SETUPZ80.CMD   Emulator command file for configure/setup
     SETUPZ80.HLP   Help file for configure/setup
     STMACZ80.HLP   Help file for standard macro commands
     HLLDZ80.DOC    Document file for high level language debug
     HLLDZ80.CMD    Emulator command file for high level language debug
     HLLDZ80.HLP    Help file for High level language debug
     CVTZ80.DOC     Document file for CVTZ80.EXE
     CVTZ80.EXE     Symbol converter executable file
     SIEVEZ.C       Sample C source file
     SIEVEZ.ABS     Sample object file

NEW FEATURE

  1. Support Continuous DUMP command

     If the end-address or length not specified, DUMP command
     displays 64 bytes of memory.

     If no parameter specified, DUMP command countinuously
     displays memory.

       d 100
       d
       d

  2. Support Continuous DISASSEMBLE command

     If no parameter specified, DISASSEMBLE command continuously
     disassembles memory.

       di 2000
       di
       di

  3. Support memory and port manipulation commands while program running

     Memory manipulation commands can be used while program is
     running.

       r reset
       go
       dump 2000
       ex 1000=0ff
